TABLE 4-3.5 STAFF/VISITORS TOILETS/ JANITOR’S CLOSET

|  |  |
| --- | --- |
| **Description/ Usage** | See Table 3-1 for Service-specific toilet requirements. These are separate male and female toilets for use by adult staff and visitors.  Navy provides multiple unisex toilets that are shared by Teens, staff, and visitors—see Table 4-9. |
| **Min. Ceiling Ht.** | 2.44 m (8 ft.) minimum. |
| **Finishes** | **Walls.**  Epoxy or enamel painted, moisture-resistant gypsum wall board with a ceramic tile wainscot. Consider full ceramic tile walls. |
|  | **Floor.** Ceramic tile. |
|  | **Ceiling.** Painted, moisture-resistant gypsum board. None needed for janitor’s closet. |
| **Plumbing** | Provide wall-hung water closets, wall-hung urinals, and lavatories based on the applicable code for the calculated occupancy. Provide a floor drain. |
| **HVAC** | 20 C (68 F) minimum, 26 C (78 F) maximum. Ventilate to the exterior per code. |
| **Fire Protection** | Provide system per paragraph 3-5.3. |
| **Power** | Provide outlets per code. |
| **Lighting** | 540 lux (50 fc). |
| **Communication** | **CCTV.** None required.  **CATV/Internal Video.** None required.  **PA/Audio.** None required.  **Telephone.** None required.  **Data.**  None required.  **Security.** Provide lockable doors. Provide a vision panel in the door. |
| **Casework** | Solid-surface countertop with either underhung or integral sink.  Solid composite toilet and urinal partitions.  Not necessary for Navy unisex toilets. |
| **Furnishings Fixtures & Equipment (FF&E)** | Toilet accessories: toilet paper dispensers, paper towel dispenser with integral trash receptacle, robe hooks, grab bars, and soap dispensers.  Mirror. |
| **Special Requirements** | Provide a Janitor’s closet associated with or in proximity of these toilets. This closet includes a mop sink with hot and cold water, a floor drain, and storage for pails, mops, vacuums, and related cleaning supplies and equipment. Include a lockable door, (which can be opened from the inside) with a vision panel. Provide lockable cabinets for cleaning supplies. Provide exhaust ventilation directly to the outside. |
| For use during project execution by the appropriate Service agency | |
| **Occupancy** | Staff. |
|  | Patrons/Youth. |
| **Min. net m2 (ft2)** |  |