TABLE 4-7.4. SPECIAL ACTIVITY ROOM

|  |  |
| --- | --- |
| **Description/ Usage** | This shared activity room is designed to be versatile and open to allow for a variety of indoor activities. As with all of the activity rooms, it is sized as a basic module to afford flexibility in use. The primary difference between this room and the General Activity Room is that it is designed for more active functions such as dance, yoga, or martial arts instruction. However, this room is not intended to accommodate team sports. |
| **Min. Ceiling Ht.** | 3.05 m (10 ft.) clear. |
| **Finishes** | **Walls.**  Painted concrete masonry unit (CMU) wall or impact-resistant gypsum wallboard (GWB) or high-density polyethylene (HDPE).  Navy and Air Force do not permit CMU in these spaces. |
|  | **Floor.** Varies depending on intended functions, but may include hard-wood dance floor, athletic flooring, etc. |
|  | **Ceiling.** ACP. |
| **Plumbing** | None required. |
| **HVAC** | 20 C (68 F) minimum, 26 C (78 F) maximum. Consider the active functions with regard to air changes and humidity control. |
| **Fire Protection** | Provide system per paragraph 3-5.3. |
| **Power** | Provide outlets per code. |
| **Lighting** | 540 lux (50 fc). |
| **Communication** | **CCTV.** Provide at least one outlet.  **CATV/Internal Video.** None required.  **PA/Audio.** Provide a speaker.  **Telephone.** Provide one line with internal two-way communication.  **Data.**  Consider providing at least two outlets.  **Security.** Do not create corners or “nooks” that are not visible from other areas of the room. |
| **Casework** | Varies depending on intended functions, but may include a segmented, height-adjustable dance (ballet) bar; full-height, shatter-proof mirrors; etc. |
| **Furnishings Fixtures & Equipment (FF&E)** | Varies depending on intended functions, but may include resilient athletic flooring, martial arts equipment, and other specialized equipment to suit the selected function. |
| **Special Requirements** | Include vision panels in interior doors and large windows in the interior walls. Provide exterior doors to outside activity area.  Army requires exterior doors to be alarmed. The Navy does not require exterior doors.  Provide a dedicated storage closet (included in the space program).  Consider acoustical requirements for these active function rooms.  Consider providing a folding room partition. |
| For use during project execution by the appropriate Service agency | |
| **Occupancy** | Staff. |
|  | Patrons/Youth. |
| **Min. net m2 (ft2)** |  |