|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ENTRY CANOPY** | | | | |
| Space Characteristics | | | | |
| **Function:** Entry Canopy  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 11’-4”  **Acoustics:**  **Access:** Exterior  **Number of Occupants:** 0  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| B201009 | Exterior Painting |  |  |  |
| F101090 | Column Supported Canopy |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **VESTIBULE** | | | | |
| Space Characteristics | | | | |
| **Function:** Vestibule  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 11’-4”  **Acoustics:**  **Access:** Vestibule  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| B203002 | Half Glass Insulated Hollow Metal Exterior Door |  |  |  |
| C101001 | Fixed Partitions |  |  |  |
| C102001 | Standard Interior Doors |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| C103014 | Recessed entry grille |  |  |  |
| C302010 | Hardeners and Sealers |  |  |  |
| [C303090] | [Concrete Ceiling Finish] |  |  | [See C304002] |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| [C304007] | [Special Coatings] |  |  |  |
| E101005 | G5 Security Vault Door with Day Gate |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **COVERED CLEANING AREA** | | | | |
| Space Characteristics | | | | |
| **Function:** Covered Cleaning Area  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height:  **Acoustics:**  **Access:** Exterior  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| [B201009] | [Painted Metal Ceiling] |  |  |  |
| C302010 | Hardeners and Sealers |  |  |  |
| D201006 | Drinking fountain |  |  |  |
| D201090 | Emergency Shower and Eyewash |  |  |  |
| D209005 | Air Compressors |  | Size accord to facility | Use outdoor type compressors |
| E109090 | Fixed Weapons Cleaning Tables |  |  | Weapons cleaning at 10 GSF per person (see the P-80) – approximately six (6) LF per person for weapons cleaning (Shown here, cleaning for one platoon (38 people) at one time) Minimum [40 inches] wide by 36 inches height |
| E109090 | Steam Cleaner |  |  | Electric and water connections |
| E109090 | Portable Solvent Cleaner |  |  | Electrical connection |
| E109090 | Weapons Clearing Discharge Canister |  |  |  |
| F101090 | Column Supported Canopy |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CORRIDOR** | | | | |
| Space Characteristics | | | | |
| **Function:** Corridor  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 11’-4”  **Acoustics:**  **Access:** Vestibule  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| C101001 | Fixed Partitions |  |  |  |
| C102001 | Standard Interior Doors |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| C103007 | Fire extinguisher cabinet |  |  |  |
| C302010 | Hardeners and Sealers |  |  |  |
| [C303090] | [Concrete Ceiling Finish] |  |  | [See C304002] |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| [C304007] | [Special Coatings] |  |  |  |
| E202003 | Metal Desk |  |  | 30 x 60 desk for door guard with writing shelf for signing in |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **WEAPONS REPAIR AND MAINTENANCE WORKSHOPS** | | | | |
| Space Characteristics | | | | |
| **Function:** Weapons Repair and Maintenance Workshops  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 11’-4”  **Acoustics:**  **Access:** Corridor  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| C101001 | Fixed Partitions |  |  |  |
| C102001 | Standard Interior Doors |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| C103008 | Solid Surface Countertop with Backsplash |  |  |  |
| C103009 | Laminate Surface Base Cabinet |  |  |  |
| C103009 | Laminate Surface Wall Cabinets |  |  |  |
| C302010 | Hardeners and Sealers |  |  |  |
| [C303090] | [Concrete Ceiling Finish] |  |  | [See C304002] |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| [C304007] | [Special Coatings] |  |  |  |
| D201004 | Stainless Steel Single Bowl |  |  |  |
| D201090 | Emergency Shower and Eyewash |  |  |  |
| D502002 | Task Lighting |  |  |  |
| D503005 | Security System |  |  | Provide panic button at each issue port |
| E103004 | Workbench |  |  |  |
| E109002 | Microwave |  |  |  |
| E109002 | Refrigerator |  |  |  |
| E109090 | Weapons Discharge Canister |  |  |  |
| E109090 | Electric Cord Reels |  |  |  |
| E202003 | Stool Height Task Seating with Adjustable Height and Backs on Casters |  |  | Molded plywood seats and backs |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **DUTY OFFICE** | | | | |
| Space Characteristics | | | | |
| **Function:** Duty Office  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 8’-0”  **Acoustics:**  **Access:** Corridor  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| C101001 | Fixed Partitions |  |  |  |
| C102001 | Standard Interior Doors |  |  |  |
| C102001 | Interior Steel door |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| E101005 | G5 Vault Door |  |  |  |
| E202002 | Modular Workstation |  |  |  |
| E202003 | Desk Chair |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UNIT ARMS ROOMS / WEAPONS STORAGE AREA** | | | | |
| Space Characteristics | | | | |
| **Function:** Unit Arms Rooms / Weapons Storage Area  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 11’-4”  **Acoustics:**  **Access:** Vestibule / Weapons Repair and Maintenance Workshops  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| B203090 | Issue Port |  |  | See drawings for issue port details, Appendix C |
| C101001 | Fixed Partitions |  |  |  |
| C101002 | Equipment Cage |  |  | 3080 cage door with push button / key lock |
| C102001 | Standard Interior Doors |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| C302010 | Hardeners and Sealers |  |  |  |
| [C303090] | [Concrete Ceiling Finish] |  |  | [See C304002] |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| [C304007] | [Special Coatings] |  |  |  |
| D503005 | Security System |  |  | Provide panic button at each issue port |
| E109090 | Weapons Racks |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **MECHANICAL ROOM** | | | | |
| Space Characteristics | | | | |
| **Function:** Mechanical Room  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 11’-4”  **Acoustics:**  **Access:** Exterior  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| C101001 | Fixed Partitions |  |  |  |
| C102001 | Standard Interior Doors |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| C302010 | Hardeners and Sealers |  |  |  |
| [C303090] | [Concrete Ceiling Finish] |  |  | [See C304002] |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| D202003 | Backflow Preventer |  |  | Special certification requirements |
| D402001 | Fire Protection Water Piping and Equipment |  |  | Fire protection equipment may require separate room |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **STAFF TOILETS /SHOWERS** | | | | |
| Space Characteristics | | | | |
| **Function:** Staff Toilets / Showers  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 8’-0”  **Acoustics:**  **Access:** Corridor  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| C101001 | Fixed Partitions |  |  |  |
| C102001 | Standard Interior Doors |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| C103001 | Toilet partition and urinal screen |  |  | Solid plastic |
| C103002 | Toilet Accessories |  |  | Toilet paper holder, grab bars, paper towel dispenser – disposer, soap dispenser, mirror with shelf |
| C103002 | Shower Curtain Rod |  |  | Across opening to shower |
| C103005 | Lockers |  |  |  |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| D201005 | Conventional Shower Enclosure |  |  | With rod and curtain. Provide accessible shower with seat, hand shower, grab bars, curtain and rod |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ELECTRICAL CLOSET** | | | | |
| Space Characteristics | | | | |
| **Function:** Electrical Closet  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 11’-4”  **Acoustics:**  **Access:** Exterior  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| C101001 | Fixed Partitions |  |  |  |
| C102001 | Standard Interior Doors |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| C302010 | Hardeners and Sealers |  |  |  |
| [C303090] | [Concrete Ceiling Finish] |  |  | [See C304002] |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| D5010 | Electrical Equipment |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **COMMUNICATIONS ROOM** | | | | |
| Space Characteristics | | | | |
| **Function:** Communications Room  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 11’-4”  **Acoustics:**  **Access:** Corridor  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| C101001 | Fixed Partitions |  |  |  |
| C102001 | Standard Interior Doors |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| C302010 | Hardeners and Sealers |  |  |  |
| [C303090] | [Concrete Ceiling Finish] |  |  | [See C304002] |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| D5030 | Communications Equipment |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **JANITOR CLOSET** | | | | |
| Space Characteristics | | | | |
| **Function:** Janitor Closet  **Special Dimensions:**  Ideal Plan Dimensions:  Minimum Ceiling Height: 8’-0”  **Acoustics:**  **Access:** Corridor  **Number of Occupants:**  **Other/special requirements:** | | | | |
| Uniformat Section | **Description** | **Qty** | **Size** | **Specific Requirements** |
| C101001 | Fixed Partitions |  |  |  |
| C102001 | Standard Interior Doors |  |  |  |
| C102001 | Solid door |  |  |  |
| C102007 | Interior Door Hardware |  |  |  |
| C102007 | Storage lockset |  |  |  |
| C103006 | Steel shelving |  |  |  |
| C302010 | Hardeners and Sealers |  |  |  |
| [C303090] | [Concrete Ceiling Finish] |  |  | [See C304002] |
| [C304002] | [Concrete Wall Finish] |  |  |  |
| [C304003] | [Concrete Masonry Finish] |  |  |  |
| D201004 | Mop Sink with Mop Hangar |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |