|  |
| --- |
| **Shock, Arc Flash, and Arc Blast Hazard**  **Appropriate PPE Required** |

**3’ - 10” Arc Flash Boundary**

**4.8 cal/cm2 Arc Flash Hazard at 18 Inches**

**8 Minimum Arc Rating of Clothing (cal/cm2)**

**480 volts Shock Hazard When Cover is Removed**

**3’ - 6” Limited Approach Boundary**

**1’ - 0” Restricted Approach Boundary**

**Equipment Name: B501D-2H2 Date: August 1, 2014**

**WARNING**