|  |
| --- |
| **Energized Work Is Not Allowed**  **Shock, Arc Flash, and Arc Blast Hazard**  **Arc flash available incident energy is**  **greater than 40 cal/cm2 at 18 inches. Failure to Comply**  **Can Result in Injury or Death.** |
|  |

**WARNING**