TABLE 4-3.4. OPTIONAL STAFF LOCKER AREA

|  |  |
| --- | --- |
| **Description/ Usage** | This optional area is used by all staff for the storage of personal articles only. It is not intended as a rest room or shower facility. It is usually part of or adjacent to the Break/Staff Training room (see Table 4-3.2). |
| **Min. Ceiling Ht.** | 2.44 m (8 ft.) minimum. |
| **Finishes** | **Walls.**  Painted gypsum wallboard or vinyl wall covering. |
|  | **Floor.** VCT with vinyl or rubber base. |
|  | **Ceiling.** ACP. |
| **Plumbing** | None required. |
| **HVAC** | 20 C (68 F) minimum, 26 C (78 F) maximum. |
| **Fire Protection** | Provide system per paragraph 3-5.3. |
| **Power** | Provide outlets per code. |
| **Lighting** | 540 lux (50 fc). |
| **Communication** | **CCTV.** None required.  **CATV/Internal Video.** None required.  **PA/Audio.** Provide a speaker.  **Telephone.** None required.  **Data.**  None required.  **Security.** None required. |
| **Casework** | None required. |
| **Furnishings Fixtures & Equipment (FF&E)** | Half-sized lockers with key/combination locks.  Navy requires padlock lockers |
| **Special Requirements** | If this is a dedicated room with a door, provide a vision panel in the door. |
| For use during project execution by the appropriate Service agency | |
| **Occupancy** | Staff. |
|  | Patrons/Youth. |
| **Min. net m2 (ft2)** |  |