TABLE 4-7.6 OPTIONAL PARENT WAITING AREA

|  |  |
| --- | --- |
| **Description/ Usage** | This optional space is in addition to the lobby waiting area and provides a comfortable area for family and friends to view youth participating in the individual programs. This area should have visual access at a minimum into the Special Activity Rooms.  Navy does not permit this optional area. |
| **Min. Ceiling Ht.** | 2.44 m (8 ft.). |
| **Finishes** | **Walls.**  Painted gypsum wallboard or vinyl wall covering. |
|  | **Floor.** Carpet with vinyl or rubber base. |
|  | **Ceiling.** ACP. |
| **Plumbing** | None required. |
| **HVAC** | 20 C (68 F) minimum, 26 C (78 F) maximum. |
| **Fire Protection** | Provide system per paragraph 3-5.3. |
| **Power** | Provide outlets per code. |
| **Lighting** | 540 Lux (50 ft. candles). |
| **Communication** | **CCTV.** Provide at least one outlet.  **CATV/Internal Video.** None required.  **PA/Audio.**  Provide a speaker.  **Telephone.** None required.  **Data.**  None required.  **Security.** None required. |
| **Casework** | None required. |
| **Furnishings Fixtures & Equipment (FF&E)** | Soft padded furniture for seating/waiting area, tables, magazine-rack. |
| **Special Requirements** |  |
| For use during project execution by the appropriate Service agency | |
| **Occupancy** | Staff. |
|  | Patrons/Youth. |
| **Min. net m2 (ft2)** |  |