TABLE 4-5.3. SNACK BAR/EATING/VENDING AREA

|  |  |
| --- | --- |
| **Description/ Usage** | This area provides the snack and beverage service for the center. It may have various configurations depending on the Service branch, size of facility, and types of programs offered.  The snack bar is a service counter that offers a limited menu such as chips, sandwiches, and sodas.   Vending supports the snack area with a limited selection of food and beverages. There are usually no more than three vending machines in a youth facility.  The Navy normally does not provide a vending area.  The eating area is directly adjacent to these functions and is part of the Commons. Seating should be comfortable and easily arranged. Consider two- and four-top tables. |
| **Min. Ceiling Ht.** | 2.44 m (8 ft.) minimum with the eating area complying with the requirements of the Commons. |
| **Finishes** | **Walls.**  Ceramic wall tile or other hard surfaces approved for the snack bar to a minimum of 1.22 m (4 ft.) from finished floor. |
|  | **Floor.** Provide hard-surface flooring such as VCT, seamless vinyl, or quarry tile or other durable material. |
|  | **Ceiling.** ACP or painted gypsum board. |
| **Plumbing** | Two-compartment countertop sink with hot and cold water supply. Floor drain. If an ice-maker is desired, provide a cold-water connection |
| **HVAC** | 20 C (68 F) minimum, 26 C (78 F) maximum. |
| **Fire Protection** | Provide system per paragraph 3-5.3. |
| **Power** | Provide dedicated outlets for the vending machines and countertop height convenience outlets for microwave and other equipment as required. |
| **Lighting** | 430 lux (40 fc) general ambient lighting. Provide task lighting. Consider accent fixtures and lighting to provide special ambience. |
| **Communication** | **CCTV.**  Provide sufficient quantity to allow adequate coverage.  **CATV/Internal Video.** None required.  **PA/Audio.**  Provide a speaker and intercom connection.  **Telephone.** None required.  **Data.**  Provide one outlet.  **Security.** None required. |
| **Casework** | Countertop with base and wall cabinets at the front opening. Behind the service corridor, provide base and wall cabinets. Countertop at sink area to be solid-surface.  Drink rail. |
| **Furnishings Fixtures & Equipment (FF&E)** | Under cabinet or counter microwave, refrigerator, freezer, and other small appliances as required. Also provide a menu board.  Vending machines.  Tables and chairs/stools in the eating area.  Consider an icemaker. |
| **Special Requirements** | Provide a roll-up door for the snack bar. |
| For use during project execution by the appropriate Service agency | |
| **Occupancy** | Staff. |
|  | Patrons/Youth. |
| **Min. net m2 (ft2)** | Snack Bar. Eating Area. |